# When I have to go through larger puddles I always put the clutch in (so that the TB closes) and just coast through if I can... nm

Posted by James (VE 5spd ) on September 16, 2004 at 16:37:08: In Reply to: How long do I have to wait until I can start my car after driving through water and stalling it out? posted by RosenKen on September 16, 2004 at 14:07:46: : Ok, blond moment I guess. Other cars were getting through about 6" water, I figured I could. But lowered car with 4 guys and a CAI (forgot about that) = stalled car. : The starter would turn but it just goes PMPH = hydrolocked I suppose. Gotta wait a day or two I guess? Stick a hair dryer up the throttle body? Would it help to hold the throttle open with a brick or something? Damn hurricanes! Replys:

Name: |
E-Mail |
Car: |
Subject |
Message:
: : Ok, blond moment I guess. Other cars were getting through about 6" water, I figured I could. But lowered car with 4 guys and a CAI (forgot about that) = stalled car. : : The starter would turn but it just goes PMPH = hydrolocked I suppose. Gotta wait a day or two I guess? Stick a hair dryer up the throttle body? Would it help to hold the throttle open with a brick or something? Damn hurricanes!