# Or you can do what I did (if you don't own a press) and pay a shop to press them in. I think I got charged $15. n/m

Posted by Pervis Anathema (91 SE) on September 08, 2004 at 19:19:52: In Reply to: on the front bushings, you can cut the outer piece and peel a notch out- like a backwards banana kinda. it comes out easier that way. --> posted by Matt on September 08, 2004 at 18:12:06: : for putting them in, the best way is to throw the control arm in the oven and the bushing in the freezer. then press them together and try not to burn/freeze yourself. Replys:

Name: |
E-Mail |
Car: |
Subject |
Message:
: : for putting them in, the best way is to throw the control arm in the oven and the bushing in the freezer. then press them together and try not to burn/freeze yourself.