# yes, if I were to drill/melt out all the rubber the inner metal sleeve would be stuck on

Posted by MrGone (92se) on September 15, 2004 at 22:34:40: In Reply to: what do u see...the inner metal sleeve stuck on? posted by DanNY on September 15, 2004 at 22:19:02: I'm thinking maybe I can take the gusset off the car put the LCA in a vise then bang the gusset part out. Haven't figured out how to use the truck on this yet :( hehehehhe ;) : i had to split mine and peel it back like a banana. : you can always use the truck's bumper to press it out..LOL :wall: Replys: wrap chain around LCA. tie to truck bumper. drive away. ;) --> Matt (93SE) 07:30:13 9/16/2004 (0) yeah burn the rubber out and then use a dremel to slice the thing and peel it back like D said nm lophix (94se) 22:44:19 9/15/2004 (3) okie I'll give that a shot MrGone (92se) 23:00:22 9/15/2004 (2) what's the worst that could happen? lophix (94se) 23:56:36 9/15/2004 (1) the roof...the roof...the roof is on fireeee! :) nm DanNY (91SE) 08:36:16 9/16/2004 (0)

Name: |
E-Mail |
Car: |
Subject |
Message:
: I'm thinking maybe I can take the gusset off the car put the LCA in a vise then bang the gusset part out. : Haven't figured out how to use the truck on this yet :( hehehehhe ;) : : i had to split mine and peel it back like a banana. : : you can always use the truck's bumper to press it out..LOL :wall: