# Nice: I'd use a heatgun to accelerate the water out of the cyls, and use WD-40, made to displace water and protect metal. Small rust spots will rub off, but will lead to early oil consumption. n/m

Posted by John vdP (93 SE) on September 17, 2004 at 07:35:23: In Reply to: Good news (so far) posted by RosenKen on September 16, 2004 at 20:03:32: .. Replys:

Name: |
E-Mail |
Car: |
Subject |
Message:
: ..