# pour some oil (tablespoon or so) into each cylinder and crank some more.. -->

Posted by Matt (93SE) on September 16, 2004 at 21:49:21: In Reply to: Good news (so far) posted by RosenKen on September 16, 2004 at 20:03:32: the last thing you want to do is get a ton of rust on the cylinder walls. coating the top of the piston in oil and splashing it around in there should help keep it from really scarring anything up. I would highly suggest using a rubber hose and sucking any water you can out. once you've got that much out, you can likely just put the plugs back in and fire it up. the rest of the water will burn off. Replys: If he's running the engine, isn't there oil in there already? n/m Jeff92se (92se) 10:02:48 9/17/2004 (2) yeah, but its in the pan, right? this way its nice fresh oil straight to each cylinder. n/m mentat (93se 5spd) 10:54:12 9/17/2004 (1) Not sure how much H20 could work it's way past the cylinder rings Jeff92se (92se) 11:18:54 9/17/2004 (0)

Name: |
E-Mail |
Car: |
Subject |
Message:
: the last thing you want to do is get a ton of rust on the cylinder walls. coating the top of the piston in oil and splashing it around in there should help keep it from really scarring anything up. : I would highly suggest using a rubber hose and sucking any water you can out. once you've got that much out, you can likely just put the plugs back in and fire it up. the rest of the water will burn off.