# Okay, my first VE question/problem

Posted by blackandwhite ('93 SE 5spd) on June 24, 2002 at 18:01:43:

Sometimes while driving, my car will stop accerelating, then when the tach needle drops below 2500 rpm it starts to sputter and jerk, the needle jumps back and forth between 2000 and 2500, but wont go past 2500 in any gear.
Then after it goes away a while (varies) and returns to normal operation. Upon a previous suggestion, I changed the fuel filter, but it didn't help.

Any Suggestions?

Replys:

- One of the things to check is the coil abdul (90 GXE 92 SE) 18:14:26 6/24/2002 (0)
- Coil packs.. Maximamike (92 SE) 18:03:51 6/24/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: Sometimes while driving, my car will stop accerelating, then when the tach needle drops below 2500 rpm it starts to sputter and jerk, the needle jumps back and forth between 2000 and 2500, but wont go past 2500 in any gear. : Then after it goes away a while (varies) and returns to normal operation. Upon a previous suggestion, I changed the fuel filter, but it didn't help. : Any Suggestions?