# One of the things to check is the coil

Posted by abdul (90 GXE 92 SE) on June 24, 2002 at 18:14:26:

In Reply to: Okay, my first VE question/problem posted by blackandwhite on June 24, 2002 at 18:01:43:

pack itself. Take them out one by one and measure their ohm rating. Mine was 0.9 ohms for all six..as long as they don't go past 1.1 or 1.2 if I recall correctly. Check the power valve solenoid. look under the throttle body, there are 2 solenoids with wires going into them, one is brown, and the other is green. Make sure it is plugged in and working..to test them plug in 12 volts and make sure they click. Under load, the car activates that valve and if it does not work, your description is one of the symptoms.

I'm assuming you checked, if not already, the spark plugs, the fuel pump/relay and residual pressure, eng cont relay (green relay in box) and other things that slip my mind who other members might be able to add to. My car is currently in the shop, throttle body and iacv valve disassembled, getting a full cleanup. I'm waiting on a gasket to assemble them. My issue is delayed cranking for about 5 seconds before the car starts. Good luck with your problem. If you need any diagrams, I have access to alldata. I can try to help you out.

Abdul

Replys:

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: pack itself. Take them out one by one and measure their ohm rating. Mine was 0.9 ohms for all six..as long as they don't go past 1.1 or 1.2 if I recall correctly. Check the power valve solenoid. look under the throttle body, there are 2 solenoids with wires going into them, one is brown, and the other is green. Make sure it is plugged in and working..to test them plug in 12 volts and make sure they click. Under load, the car activates that valve and if it does not work, your description is one of the symptoms. : I'm assuming you checked, if not already, the spark plugs, the fuel pump/relay and residual pressure, eng cont relay (green relay in box) and other things that slip my mind who other members might be able to add to. My car is currently in the shop, throttle body and iacv valve disassembled, getting a full cleanup. I'm waiting on a gasket to assemble them. My issue is delayed cranking for about 5 seconds before the car starts. Good luck with your problem. If you need any diagrams, I have access to alldata. I can try to help you out. : Abdul