# you dont need to run new wires

Posted by Craig B (93 SE) on June 15, 2002 at 19:23:55:

In Reply to: Dumping the BOSE posted by mverse on June 15, 2002 at 19:09:49:

I'm not sure if 4th gens are different or maybe Turbo97 is just trying to confuse people (he does that sometimes)

If you just us the stock wiring from the head unit harness to the speakers, and then unplug them from the amps like I mentioned on my page, you'll be fine

I really dont think the fronts are 6.5" They are round, but I dont think they're that big, maybe closer to 5" if that. I put some custom wood panels in there with some 4x6 speakers.

Replys:

- the fronts are around 4 inches, however you can prolly fit a shallow 8inch sub in there nm, Alex (90se5spd) 20:10:41 6/15/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: I'm not sure if 4th gens are different or maybe Turbo97 is just trying to confuse people (he does that sometimes) : If you just us the stock wiring from the head unit harness to the speakers, and then unplug them from the amps like I mentioned on my page, you'll be fine : I really dont think the fronts are 6.5" They are round, but I dont think they're that big, maybe closer to 5" if that. I put some custom wood panels in there with some 4x6 speakers.