# Re: When grounding VTC, is there only one wire (inside of the sheath) going to the solenoid?

Posted by Evil Yak (93SE) on June 17, 2002 at 13:00:58:

In Reply to: When grounding VTC, is there only one wire (inside of the sheath) going to the solenoid? posted by Maximax on June 17, 2002 at 12:47:03:

there should be two...
a red/black and something else
don't ground the red/black... that's your ignition wire

Replys:

- Thanks, soon to be tick free......nm. Maximax (93.SE.5SP) 14:32:25 6/17/2002 (0)
- yellow/green is the other Craig B (93 SE) 13:45:05 6/17/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: there should be two... : a red/black and something else : don't ground the red/black... that's your ignition wire