# Dude way to complicated. Do this..........

Posted by 89 SE 5spd (89 SE 5spd) on June 19, 2002 at 20:22:21:

In Reply to: Selt Belt Chime jump instructions? posted by PaxMax on June 19, 2002 at 11:18:31:

The damn chime is on the back of the Gauge cluster. You cant miss it. I did this when I swapped clusters. Pull your cluster out and is the big metal thing back there. It's got a positive and a ground wire and a mounting screw. Pull it out and no more annoying noise. No sense in jumping out either side of the car.

Replys:

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: The damn chime is on the back of the Gauge cluster. You cant miss it. I did this when I swapped clusters. Pull your cluster out and is the big metal thing back there. It's got a positive and a ground wire and a mounting screw. Pull it out and no more annoying noise. No sense in jumping out either side of the car.