# Remove the radio trim panel, undo the four screws around it, cut a hole in the firewall and pull it out from behind...

Posted by Uncle Pete (89 SE) on June 23, 2002 at 17:16:27:

In Reply to: A/C Controls HELP!! posted by Jonathan on June 23, 2002 at 16:57:19:

Yes, yes - I'm joking of course. I was discussing this with Craig a few days ago. The only times I've had them out is when I've been removing the whole dashboard to get the heater core. We think that if you remove the radio and stupid compartment you might get it out by removing the mounting screws and dropping it down through the radio hole. Bear in mind that unless you have the auto climate control there will be a physical cable connection that you will have to unhook from the heat exchange unit.

Replys:

- yes you can pull it down through the radio hole...I did that once.nm awsm66 (93SE) 21:11:25 6/23/2002 (0)
- Oh shoot! You ere kidding???? Oops!... Jonathan (Mighty Max 94SE) 17:20:03 6/23/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: Yes, yes - I'm joking of course. I was discussing this with Craig a few days ago. The only times I've had them out is when I've been removing the whole dashboard to get the heater core. We think that if you remove the radio and stupid compartment you might get it out by removing the mounting screws and dropping it down through the radio hole. Bear in mind that unless you have the auto climate control there will be a physical cable connection that you will have to unhook from the heat exchange unit.