# RSB end link broke of the frame enh? two ways to fix it..

Posted by DanNY (91SE) on June 26, 2002 at 08:26:20:

In Reply to: WAHH! posted by Alex on June 26, 2002 at 08:24:37:

the very very temp way..
get a big washer and put in between the frame piece..bolt on link tight.
that would sandwich them together for now.

the perm way...
get a piece of steel..bust out the welder. enjoy.

:

Replys:

- Re: RSB end link broke of the frame enh? two ways to fix it.. DaBoxSE (93SE 5spd-RIP 91SE 5spd) 09:19:28 6/26/2002 (2)
  - yulp! nm DanNY (91SE) 09:27:01 6/26/2002 (1)
    - Re: yulp! nm MIKE (93VE) 19:16:52 6/27/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: the very very temp way.. : get a big washer and put in between the frame piece..bolt on link tight. : that would sandwich them together for now. : the perm way... : get a piece of steel..bust out the welder. enjoy. : : : <img src=http://lcs.mlin.net/temp/DSCF0655.JPG>