# open -->

Posted by Bryan (91 SE, 92 SE) on July 02, 2002 at 22:11:20:

In Reply to: changing the tranny fluid???? how to... posted by Steve on July 02, 2002 at 21:35:37:

http://members.csinet.net/tisch/maxima/faq.htm#transmission delay

Just drain and replace. Read the above link first. You have a VG, so only about 3 quarts will come out. Use a 1/2 inch ratchet to loosen the drain plug.

Replys:

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: http://members.csinet.net/tisch/maxima/faq.htm#transmission delay : : Just drain and replace. Read the above link first. You have a VG, so only about 3 quarts will come out. Use a 1/2 inch ratchet to loosen the drain plug.