# Bret....

Posted by DA-MAX (91 GXE) on July 03, 2002 at 16:26:48:

In Reply to: Power valve actuator was disconnected!! (more) posted by Bret on July 03, 2002 at 16:06:07:

any ideas on the entire power valve assembly removal??? I think the actual actuator part has developed a leak...(evidence from the whinning noise it is making). looks like just unscrew and replace, any ideas

Replys:

- It's easy. 2 or 3 screws (you'll need a #3 phillips and some elbow grease though) and an e-clip on the end of the shaft. 5-10 min job to replace.. --> Matt (93SE) 16:29:03 7/03/2002 (1)
  - LOL...I was just about to ask if you had it! thanks man! :-) nm DA-MAX (91 GXE) 16:31:05 7/03/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: any ideas on the entire power valve assembly removal??? I think the actual actuator part has developed a leak...(evidence from the whinning noise it is making). looks like just unscrew and replace, any ideas