# STEP #1!!! PULL THE FUSE OUT! It'll keep it from doing any more damage. -->

Posted by Matt (93SE) on July 12, 2003 at 14:20:53: In Reply to: Before you go shopping in Crutchfield posted by MIKE on July 12, 2003 at 11:46:51: once you get time to mess with it, pull the head unit out and pull the covers off. look where the stuff spilled in it and do your best to clean it up with contact cleaner. Be careful not to get it on the laser part of the CD though, as those laser heads are a PIA to clean. you've got nothing to lose, right? :) Replys:

Name: |
E-Mail |
Car: |
Subject |
Message:
: once you get time to mess with it, pull the head unit out and pull the covers off. look where the stuff spilled in it and do your best to clean it up with contact cleaner. : Be careful not to get it on the laser part of the CD though, as those laser heads are a PIA to clean. : you've got nothing to lose, right? :)