# Yeah, I got it. This is a "tomorrow after work" job. I love having 2 cars!!! :) n/m

Posted by unsigned (92SE/89GXE) on July 15, 2003 at 00:00:20: In Reply to: You have to find TDC posted by Nismo87se on July 14, 2003 at 22:32:42: : I had some issues with mine too. What you have to do is line up the TDC mark on the crank pulley wiht the pointer and hope it is on the intake stroke. Then you have to line up the dot on the dizzy gear with a slash mark on the housing. AFter that once you put the dizzy in the engine will be on the right timing, so you'll be able to set it after that. Replys:

Name: |
E-Mail |
Car: |
Subject |
Message:
: : I had some issues with mine too. What you have to do is line up the TDC mark on the crank pulley wiht the pointer and hope it is on the intake stroke. Then you have to line up the dot on the dizzy gear with a slash mark on the housing. AFter that once you put the dizzy in the engine will be on the right timing, so you'll be able to set it after that.