# correct on the work required.. the whole rail comes out at once, then you replace injectors as needed -->

Posted by Matt (93SE) on July 08, 2003 at 10:49:45: In Reply to: More info posted by Black Max on July 08, 2003 at 06:47:32: I didn't read the rest of the thread, but have you tried using any fuel system cleaners yet? they don't really "dry out", but what they will do is get gunky deposits in the tips and clog them up. they'll still read the proper resistance and sound like they're working, but they just won't spray. I ran into a problem with that last week on another guy's VG... time to clean them out and see what happens! Replys: That is what happened to my injectors. Resistance was fine. Turned out that the tips were full of black gunk. n/m Pervis Anathema ('91 SE) 18:24:01 7/08/2003 (0) yes, definitely try this first n/m Bryan (fmr 91,92 SE) 15:00:48 7/08/2003 (0)

Name: |
E-Mail |
Car: |
Subject |
Message:
: I didn't read the rest of the thread, but have you tried using any fuel system cleaners yet? they don't really "dry out", but what they will do is get gunky deposits in the tips and clog them up. they'll still read the proper resistance and sound like they're working, but they just won't spray. I ran into a problem with that last week on another guy's VG... time to clean them out and see what happens!