# Disagree

Posted by Mike S. (93gxe) on July 11, 2003 at 14:42:06: In Reply to: I don't thing a 02 has the ability to cause a problem in a specific rpm range n/m posted by Jeff92se on July 11, 2003 at 13:26:58: When my o2 got damaged I got really nasty hesitation at around 1-1.5K. It only happened when you first started the car in the morining. Also, even after the car had been running it would act funny. If I was coasting to a stop (4th gear auto) around 30mph the car is just floating around 900rpm(thats normal), but it would almost cut out and drop to 600 than back up to 1000. O2 fixed my problem. I figured it had to be because I never had any probs, then i my y pipe installed and it started to happen as i pulled out of the driveway of the installer. Mike S. Replys: Please explain in technical terms how an 02 sensor can cause a rpm specifc problem not a whole rpm problem that's excerbated in the 1.5k rpm range n/m Jeff92se (92se) 14:45:46 7/11/2003 (1) I can't, but I'm not going to beat this like a dead horse..... Mike S. (93gxe) 17:31:42 7/11/2003 (0)

Name: |
E-Mail |
Car: |
Subject |
Message:
: When my o2 got damaged I got really nasty hesitation at around 1-1.5K. It only happened when you first started the car in the morining. Also, even after the car had been running it would act funny. If I was coasting to a stop (4th gear auto) around 30mph the car is just floating around 900rpm(thats normal), but it would almost cut out and drop to 600 than back up to 1000. : O2 fixed my problem. I figured it had to be because I never had any probs, then i my y pipe installed and it started to happen as i pulled out of the driveway of the installer. : Mike S.