# Finally got the tokico's and eibach's installed, took a little longer than expected -->

Posted by Isaacm (94 SE) on September 03, 2002 at 11:45:12:

All went fine, until the last struts - rear drivers side. The rear sway bar bushing bolt would not loosen, it just twisted the bushing around as far as it could go. So, obviously the bushing is shot. It looks to be a press fit. Probably a good time to upgrade the rear sway bar. Any ideas to get the bolt out?

Replys:

- i had a similar problem when i did the latest spring swap... Chris91se (91se) 12:32:26 9/03/2002 (0)
- Uhhh, shouldn't it unscrew from the bracket on the bottom of the strut? nm Matt (93SE) 11:53:03 9/03/2002 (2)
  - Sorry I didn't explain better...--> Isaacm (94 SE) 12:29:58 9/03/2002 (1)
    - I've gotten your emails, just too busy/lazy to reply. --> Matt (93SE) 12:36:54 9/03/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: All went fine, until the last struts - rear drivers side. The rear sway bar bushing bolt would not loosen, it just twisted the bushing around as far as it could go. So, obviously the bushing is shot. It looks to be a press fit. Probably a good time to upgrade the rear sway bar. Any ideas to get the bolt out?