# Sorry, this is for the metal sheet where the resonator pipe currently goes down into. n/m

Posted by The Max (92 J30 Maxima (turbo project underway)) on September 04, 2002 at 05:33:21:

In Reply to: Guys, what tool should I use for the CAI pipe down the front fender? Hole saw or nibbler? n/m posted by The Max on September 04, 2002 at 05:32:49:

Replys:

- If the sheetmetal is rigid enough and you're not worried about something behind it, I'd say the holesaw. nm Albert ('97gxe) 07:11:30 9/04/2002 (4)
  - for the standard cai--> Matt K (89 SE 5spd) 11:14:58 9/04/2002 (3)
    - Argh....that bracing welded to the back is the biggest freakin pain....I had to sit there and bend it back and forth till it broke off.....nm James (2 VE's) 11:55:57 9/04/2002 (2)
      - Me too. plasma cutter if you have access to one. :) nm Matt (93SE) 13:17:17 9/04/2002 (1)
        - indeed... that was one of the billion or so times I've said, "Damn, why don't I have a plasma cutter?" Matt K (89 SE 5spd) 14:47:22 9/04/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments: