# No bad wrecks. Nothing is bent up front. Rears are like -0.9(not bad) but one of the fronts is -1.1(not horrendous but tire wear is noticable)->

Posted by Jeff92se (92se) on September 09, 2002 at 13:50:58:

In Reply to: Wreck? bent control arms? worn bushings? how far off is it? nm posted by Matt on September 09, 2002 at 13:08:52:

I've had these KUMHOS for some time now but you can tell the insides are wearing out faster than the rest of the tire.

: : : They didn't align it because of my torn axle boot, but here's the specs they got off the car from when we re-assebled the suspension. Not too bad if you ask me...

: : : Front:
: : : Camber: L: -.70 R: -.50
: : : Caster: L: +1.3 R: +1.00
: : : Toe: L: +.04 R: +.04

: : : Rear:
: : : Camber: L: -.80 R: -.80
: : : Toe: L: +.12 R: -.04

: : : Definitely need some adjustments but it's not as crazy as I was expecting. With my rear toe settings, I should be able to make some pretty crazy LH turns.

: : : -Jacob

Replys:

- I had it too, until I changed out the ball joints..since then, it's been cool. blackandwhite (93 VE 5spd) 12:26:08 9/13/2002 (0)
- Mine are close to that also, but that's easy to fix. unbolt the two bolts on the spindle, yank that sumbitch out some, then bolt it back together. there's a degree of play in the bolts. nm Matt (93SE) 01:01:29 9/10/2002 (0)
- I have the exact same issue, same suspension/tire setup as Jeff... Jonny (94se 5spd) 16:04:51 9/09/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: I've had these KUMHOS for some time now but you can tell the insides are wearing out faster than the rest of the tire. : : : : They didn't align it because of my torn axle boot, but here's the specs they got off the car from when we re-assebled the suspension. Not too bad if you ask me... : : : : Front: : : : : Camber: L: -.70 R: -.50 : : : : Caster: L: +1.3 R: +1.00 : : : : Toe: L: +.04 R: +.04 : : : : Rear: : : : : Camber: L: -.80 R: -.80 : : : : Toe: L: +.12 R: -.04 : : : : Definitely need some adjustments but it's not as crazy as I was expecting. With my rear toe settings, I should be able to make some pretty crazy LH turns. : : : : -Jacob