# What parts of the VE should be covered/taped up before blasting it with engine cleaner and the hose? obviously not the distributor but is there anything i should be careful with? n/m

Posted by mentat (93se 5spd) on September 07, 2002 at 09:33:41:

Replys:

- Your VE engine does not have a distributor.. I just used an enigne foam cleaner but I make sure that I wrap up the coils, power transistor and just about anything you don't want to get wet. Then use a very fine spray nozzle to hose it down. nm G3Max (92 SE Auto (out of commission needs a ring job) & 92 SE 5 speed) 10:49:21 9/07/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments: