# That Tial looks added on. Did you go from an internal to external? -->

Posted by Jeff92se (92se) on September 09, 2002 at 17:38:07:

In Reply to: Pics... posted by Jacob on September 09, 2002 at 17:21:10:

looks like you had to drill a big hole in the turbo flange area to get a singal to the WG. Then make a dump tube into the DP. Interesting. I might end up doing the same but for clearance reasons.

: Clicky

: -Jacob

Replys:

- Uses an adapter between the mani and turbo... Jacob ('93 SE) 17:54:08 9/09/2002 (2)
  - You can see the adapter in this pic... Jacob ('93 SE) 17:55:59 9/09/2002 (1)
    - Ah thanks. Some of the pics were taking along time to load. I can't do it that way rats n/m Jeff92se (92se) 18:04:58 9/09/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: looks like you had to drill a big hole in the turbo flange area to get a singal to the WG. Then make a dump tube into the DP. Interesting. I might end up doing the same but for clearance reasons. : : <A HREF="http://speedracer.speedtoys.com/~gemohler/celicas/motorpull/">Clicky</a> : : -Jacob