# Anything I should know when replacing the front lower control arm??

Posted by DA-MAX (91 GXE) on September 08, 2002 at 18:59:31:

had a short title bout with a curb last night, DOH!!! f'd up my rim and the left control arm is slightly bent...anyways the directoins in the Haynes manual look pretty straight forward, is there anything else I should look to do while down there?? will airtools be necessary or will the standard torque wrench do the job?? any suggestions...thanks.

Replys:

- Grab you biggest breaker bar and a pipe. n/m jim (93se-90gxe-240sx) 22:11:58 9/08/2002 (1)
  - Damn...all these "big" tools are scaring the sh*t out of me! LMAO!!!! :-) nm DA-MAX (91 GXE) 22:20:56 9/08/2002 (0)
- Be sure to get a big hammer. Make sure the car is really stable. Be sure to torque the bolts when the car is resting on tires! n/m Kaleb (Black '93 GXE 5spd) 20:52:18 9/08/2002 (0)
- holy sheeeeit DanNY (91SE) 20:44:22 9/08/2002 (0)

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: had a short title bout with a curb last night, DOH!!! f'd up my rim and the left control arm is slightly bent...anyways the directoins in the Haynes manual look pretty straight forward, is there anything else I should look to do while down there?? will airtools be necessary or will the standard torque wrench do the job?? any suggestions...thanks.