# I have the exact same issue, same suspension/tire setup as Jeff...

Posted by Jonny (94se 5spd) on September 09, 2002 at 16:04:51:

In Reply to: No bad wrecks. Nothing is bent up front. Rears are like -0.9(not bad) but one of the fronts is -1.1(not horrendous but tire wear is noticable)-> posted by Jeff92se on September 09, 2002 at 13:50:58:

I wish I still had my alignment spec sheet, they were al within spec, but some barely so. I have the same Inside tire wear on the fronts, its pretty bad, My Kumhos are only gonna last me about 2-3 more months at this rate, and ive had them for all of a year now.

: I've had these KUMHOS for some time now but you can tell the insides are wearing out faster than the rest of the tire.

: : : : They didn't align it because of my torn axle boot, but here's the specs they got off the car from when we re-assebled the suspension. Not too bad if you ask me...

: : : : Front:
: : : : Camber: L: -.70 R: -.50
: : : : Caster: L: +1.3 R: +1.00
: : : : Toe: L: +.04 R: +.04

: : : : Rear:
: : : : Camber: L: -.80 R: -.80
: : : : Toe: L: +.12 R: -.04

: : : : Definitely need some adjustments but it's not as crazy as I was expecting. With my rear toe settings, I should be able to make some pretty crazy LH turns.

: : : : -Jacob

Replys:

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: I wish I still had my alignment spec sheet, they were al within spec, but some barely so. I have the same Inside tire wear on the fronts, its pretty bad, My Kumhos are only gonna last me about 2-3 more months at this rate, and ive had them for all of a year now. : : I've had these KUMHOS for some time now but you can tell the insides are wearing out faster than the rest of the tire. : : : : : They didn't align it because of my torn axle boot, but here's the specs they got off the car from when we re-assebled the suspension. Not too bad if you ask me... : : : : : Front: : : : : : Camber: L: -.70 R: -.50 : : : : : Caster: L: +1.3 R: +1.00 : : : : : Toe: L: +.04 R: +.04 : : : : : Rear: : : : : : Camber: L: -.80 R: -.80 : : : : : Toe: L: +.12 R: -.04 : : : : : Definitely need some adjustments but it's not as crazy as I was expecting. With my rear toe settings, I should be able to make some pretty crazy LH turns. : : : : : -Jacob