# Jeff is so right about filling your tranny fluid that way, sooooooooo much easier

Posted by mentat (93se 5spd) on September 05, 2002 at 23:01:32:

In Reply to: Replace the 2 tranny output shaft seals also. It's better to drain the fluid first and--> posted by Jeff92se on September 05, 2002 at 18:23:31:

and using a relatively large plastic hose - I think I used 3/4" I.D. tubing - makes for faster flowing, filling, and spilling. measure it first like I didn't =]

Replys:

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: and using a relatively large plastic hose - I think I used 3/4" I.D. tubing - makes for faster flowing, filling, and spilling. measure it first like I didn't =]