# Nah... put a straight-edge up against the old one. If it's warped a bit, have it machined down. Did it to mine (just because), not a leak... n/m

Posted by RosenKen (93 SE 5spd) on September 13, 2002 at 20:09:55:

In Reply to: What studs are we posta use to replace bad ones with? Z31-T? Do I need a new manifold too? posted by Jacob on September 13, 2002 at 19:07:44:

: The last person I talked to said I need a new manifold - I imagine this is not too cheap. Anyone have any recommendations?

: I found an ex-Nissan tech who says he has done this before and can help... Maybe it will get fixed after all!

: -Jacob

Replys:

Post a Reply:

Name: |
E-Mail |
Car: |
Subject |
Comments:
: : The last person I talked to said I need a new manifold - I imagine this is not too cheap. Anyone have any recommendations? : : I found an ex-Nissan tech who says he has done this before and can help... Maybe it will get fixed after all! : : -Jacob