# Sunroof: -->

Posted by lophix (91se) on September 22, 2003 at 19:55:09: Not knowing much about the way this mechanism works, can someone please explain to me how the motor works in detail? I understand how the window motors work ( +ve on one line and -ve on the other line for up and vice versa for down). In this sense, is it correct to "assume" that pushing the "up" button sends a +ve to one line and -ve to the other to send it up...and vice versa to send it down and then reversed again to send it rolling back when the same button is pushed and the polarities are reversed once again when the forward button is pushed? (sorry for the runon words) It just kinda ticked me that i use it daily but have absolutely no idea what exactly it does or how it works. of course, i have an ulterior motive, but it definitely won't affect the running of the motor in anyway . thanks Replys: idea scrapped. i think i like holding my hand up for the 10s than figuring a way to do this. n/m lophix (91se) 01:53:16 9/23/2003 (0) yeah, pretty much.. but the problem is the two-press close.--> Matt (93SE) 22:51:04 9/22/2003 (2) shoot. forgot about that 2 step closing...nissan made that as a safety precaution, didnt they?.. lophix (91se) 01:00:16 9/23/2003 (1) I dont know «§» (93 SE) 10:44:34 9/23/2003 (0)

Name: |
E-Mail |
Car: |
Subject |
Message:
: Not knowing much about the way this mechanism works, can someone please explain to me how the motor works in detail? I understand how the window motors work ( +ve on one line and -ve on the other line for up and vice versa for down). In this sense, is it correct to "assume" that pushing the "up" button sends a +ve to one line and -ve to the other to send it up...and vice versa to send it down and then reversed again to send it rolling back when the same button is pushed and the polarities are reversed once again when the forward button is pushed? (sorry for the runon words) It just kinda ticked me that i use it daily but have absolutely no idea what exactly it does or how it works. of course, i have an ulterior motive, but it definitely won't affect the running of the motor in anyway : . thanks