# So I think I am going to polish my intake plenum...I found my old...

Posted by awsm66 (93SE) on September 23, 2003 at 19:20:35: eastwood manifold polish kit I used on my old Victor Jr. intake for my Nova. it is a kit that has different sand paper, polish compounds and bits to fit my small die grinder. I decided to test out a small spot on my spare 5spd plenum to see how well it worked. below is a picture of a small spot I sanded and polished in about 20 min. I will work on it off and on until I get it done and then clear it. Dan do you think "real" clear will hold up to the heat and not turn? I know people used to use spray can clear and it would always turn from the heat. I figure real clear would be fine though. Replys: Michael is that a 5-spd plenum? with power valve?? mentat (93se 5spd) 12:20:20 9/24/2003 (0) Yeah Eastwood has a special clear coating but I wouldn't coat it anyway if I were you. n/m Kaleb (Black '93 GXE 5spd) 09:18:58 9/24/2003 (1) i do agree w/ kaylube here..but if u MUST clear..check out the stuff i told u..nm DanNY (91SE) 11:28:51 9/24/2003 (0) It's aluminium dude. Do NOT use clear! The second it chips, you have to strip and respray. n/m The Max (92 J30 Maxima (turbo project nearing completion)) 03:04:21 9/24/2003 (0) That looks so great Mike... dmontzsta (92 SE) 22:23:29 9/23/2003 (0) Mike... Matt (93SE) 20:12:05 9/23/2003 (0) Looks nice MIKE!...great work...nm oE (Two-Tone Pimp...) 19:28:38 9/23/2003 (0)

Name: |
E-Mail |
Car: |
Subject |
Message:
: eastwood manifold polish kit I used on my old Victor Jr. intake for my Nova. : it is a kit that has different sand paper, polish compounds and bits to fit my small die grinder. : I decided to test out a small spot on my spare 5spd plenum to see how well it worked. : below is a picture of a small spot I sanded and polished in about 20 min. I will work on it off and on until I get it done and then clear it. : <img src="http://mywebpages.comcast.net/michael-h/polish/intakepolish.jpg"> : Dan do you think "real" clear will hold up to the heat and not turn? I know people used to use spray can clear and it would always turn from the heat. I figure real clear would be fine though.