# Yup.. board under oil pan. works great -->

Posted by Matt (93SE) on September 26, 2003 at 18:53:16: In Reply to: I see. Where exactly did you support the engine? --> posted by Aaron on September 26, 2003 at 18:39:45: You can try to get it off without removing the Y pipe, but I don't think you're going to be able to get to the rear engine mount without pulling it. it's either the bolts at the bottom don't have clearance before you hit the frame or the Y pipe, OR the top bolt hits the y pipe behind the engine. not sure which, but it don't work. Replys: Oh yeah, I'm doing my tranny mounts too. They might be a different story. n/m Aaron (92 SE Auto) 19:03:27 9/26/2003 (1) Nope.. swap the engine mounts, then you can pull the tranny mounts one at a time and swap them --> Matt (93SE) 20:00:56 9/26/2003 (0)

Name: |
E-Mail |
Car: |
Subject |
Message:
: You can try to get it off without removing the Y pipe, but I don't think you're going to be able to get to the rear engine mount without pulling it. : it's either the bolts at the bottom don't have clearance before you hit the frame or the Y pipe, OR the top bolt hits the y pipe behind the engine. not sure which, but it don't work.