# Damn Aaron... posting not even after an hour after we toss these ideas around??? :P

Posted by Dark Lord Bunny (89SE) on October 01, 2003 at 01:06:39: In Reply to: Alright, that's the kinda answer I was looking for... thank you so much --> posted by Aaron on September 30, 2003 at 16:32:07: Good luck with the front support... you're probably going to have to zip tie the bumper cover or something. I've torn down the front of my car enough times to know that if you don't have that bumper support... all you have are about 3-4 bolts on each side connected to the fender holding it up. : Like I said, it's just for the track, so it may work. I will test it nice so I can make sure it won't fall off halfway down the track. lol If the process is simple, then I will do it just for 26lbs of weight reduction. : Then I will look at the front support and HOPE it's the same as the rear... as far as the screws on the top. Thanks again. : : : the bottom bolts go to the support BUT the cover should be sturdy enough to be supported by the upper and sides for it not to be a problem not being connected at the bottom...just test it and see. Replys:

Name: |
E-Mail |
Car: |
Subject |
Message:
: Good luck with the front support... you're probably going to have to zip tie the bumper cover or something. I've torn down the front of my car enough times to know that if you don't have that bumper support... all you have are about 3-4 bolts on each side connected to the fender holding it up. : : Like I said, it's just for the track, so it may work. I will test it nice so I can make sure it won't fall off halfway down the track. lol If the process is simple, then I will do it just for 26lbs of weight reduction. : : Then I will look at the front support and HOPE it's the same as the rear... as far as the screws on the top. Thanks again. : : : : : the bottom bolts go to the support BUT the cover should be sturdy enough to be supported by the upper and sides for it not to be a problem not being connected at the bottom...just test it and see.