# Gives you a little bit more space, but you dont have to....nm

Posted by KLoWnPR109 (89 GXE) on October 02, 2003 at 21:15:27: In Reply to: Do you need to remove the y-pipe when replacing flywheel and clutch? n.m posted by SeaMAX on October 02, 2003 at 19:31:23: : n/m Replys: I'm glad that it's a 'semi' no because I took a look today.. SeaMAX (93 SE) 21:56:20 10/02/2003 (5) That's unpossible. no way you can get a welder around the rear Y flange. nm Matt (93SE) 22:40:25 10/02/2003 (3) I think how they did it was to let the y-pipe.. SeaMAX (93 ) 22:57:11 10/02/2003 (2) Ohhhh, so you're saying the y pipe is still bolted to the manifolds, but all other pipe is welded? nm Matt (93SE) 23:09:37 10/02/2003 (1) Exactly, that's the way my exhaust is MIKEq (93VE) 04:35:47 10/03/2003 (0) are you sure? MrGone (92se) 22:03:14 10/02/2003 (0)

Name: |
E-Mail |
Car: |
Subject |
Message:
: : n/m