# Exactly, that's the way my exhaust is

Posted by MIKEq (93VE) on October 03, 2003 at 04:35:47: In Reply to: Ohhhh, so you're saying the y pipe is still bolted to the manifolds, but all other pipe is welded? nm posted by Matt on October 02, 2003 at 23:09:37: Exhaust manifolds are bolted to heads as normal. Y-pipe is bolted to exh manifolds as normal, but from there I have no flanges. Kinda sucks for routine maintenance but that's what I got. Now looking back would I have done it different (paid more) to have flanges installed, yes. But I've been lucky so far where this hasn't been a problem. I had this done when I installed the 2.5" piping way back. Most muffler shops will pipe bend you a new exh system without any flanges and just weld on your cat and muffler unless you specify what you want. Replys:

Name: |
E-Mail |
Car: |
Subject |
Message:
: Exhaust manifolds are bolted to heads as normal. Y-pipe is bolted to exh manifolds as normal, but from there I have no flanges. Kinda sucks for routine maintenance but that's what I got. : Now looking back would I have done it different (paid more) to have flanges installed, yes. But I've been lucky so far where this hasn't been a problem. : I had this done when I installed the 2.5" piping way back. Most muffler shops will pipe bend you a new exh system without any flanges and just weld on your cat and muffler unless you specify what you want.