# The outer one (that you have) is definitely needed. the inner one should be there to help the seal last longer, but it's okay. -->

Posted by Matt (93SE) on September 27, 2003 at 10:33:57: In Reply to: I just checked....it definitely has the one on the wheel end... posted by James on September 26, 2003 at 22:54:36: It hasn't been on mine in about a year. the fun part is that the seal is covered in grease. dirt sticks to grease really well. axle turns in the same place.. dirt gets dragged into seal/axle/grease. you can see where I'm going. the outer one is where the dust seal actually rides against to provide the seal, so it must be there. Replys:

Name: |
E-Mail |
Car: |
Subject |
Message:
: It hasn't been on mine in about a year. the fun part is that the seal is covered in grease. dirt sticks to grease really well. axle turns in the same place.. dirt gets dragged into seal/axle/grease. you can see where I'm going. : the outer one is where the dust seal actually rides against to provide the seal, so it must be there.