# This doesn't require that part of remocing the ball joint. just the three 17mm nuts on the bottom. nm

Posted by Matt (93SE) on October 08, 2003 at 23:03:48: In Reply to: Even though I've read the oven trick didn't work well posted by MIKE on October 08, 2003 at 22:49:52: : Personally I would say if you dont have access to a hyd press with attachments to seperate ball joints I wouldn't tackle this job as a "home project" Take Craig advise and remove the control arms and bring them to a local shop for the bushings to be press in/out. Especially if you want the job complete in one day. I had access to a press and the job went well. Replys: I worded it incorrect MIKE (93VE) 23:14:04 10/08/2003 (1) gotcha. nm Matt (93SE) 23:29:57 10/08/2003 (0)

Name: |
E-Mail |
Car: |
Subject |
Message:
: : Personally I would say if you dont have access to a hyd press with attachments to seperate ball joints I wouldn't tackle this job as a "home project" Take Craig advise and remove the control arms and bring them to a local shop for the bushings to be press in/out. Especially if you want the job complete in one day. I had access to a press and the job went well.