# I just ordered the new EGR....where do I get the pcv....Pepboys didnt have it listed for the VE....nm

Posted by James (VE 5spd ) on October 03, 2003 at 15:04:33: In Reply to: I'd get a new egr and pcv valve. The carsound might only be a 2 way posted by Jeff92se on October 03, 2003 at 13:13:43: : so the nox might be high either way. But replace these two things first and see. : : they told me yesterday that it did pass and that the operator forgot to put the sticker on it, and to go pick the sticker up this morning. Well I go up there and turns out they didnt even inspect it..I dunno if they forgot or what. : : So they ran it this morning and it failed : : High Speed 25 mph 1685 rpm : : HC(PPM) standard is 120 it did 135 : : NOx(PPM) standard is 848 it did 2770 : : Low Speed 15 mph 1429 rpm : : HC(PPM) standard is 124 it did 219 : : NOx(PPM) standard is 937 it did 2512 : : They suggested EGR and a bad cat. The cat is about 2 yrs old it's a Carsound from WSP. I cleaned that EGR back in June and put it on the auto and it passed. : : Would it be bad this quick? Also could the cat really be bad (or I guess just doesnt perform 'street legal' like it's supposed to)? : : I guess I'm just gonna bite the bullet and buy a new EGR because I dont want to have to rig it every year to pass, but if I have to buy a cat too then that just sucks. :) : : Opinions? Replys: James about the PCV at PepBoyz MIKE (93VE) 04:23:35 10/04/2003 (0) I *might* have a new Nissan one here - if I can find it this weekend, it's yours.. nm Jacob ('03 WRX) 21:18:28 10/03/2003 (0)

Name: |
E-Mail |
Car: |
Subject |
Message:
: : so the nox might be high either way. But replace these two things first and see. : : : they told me yesterday that it did pass and that the operator forgot to put the sticker on it, and to go pick the sticker up this morning. Well I go up there and turns out they didnt even inspect it..I dunno if they forgot or what. : : : So they ran it this morning and it failed : : : <b>High Speed 25 mph 1685 rpm</b> : : : HC(PPM) standard is 120 it did 135 : : : NOx(PPM) standard is 848 it did 2770 : : : <b>Low Speed 15 mph 1429 rpm</b> : : : HC(PPM) standard is 124 it did 219 : : : NOx(PPM) standard is 937 it did 2512 : : : They suggested EGR and a bad cat. The cat is about 2 yrs old it's a Carsound from WSP. I cleaned that EGR back in June and put it on the auto and it passed. : : : Would it be bad this quick? Also could the cat really be bad (or I guess just doesnt perform 'street legal' like it's supposed to)? : : : I guess I'm just gonna bite the bullet and buy a new EGR because I dont want to have to rig it every year to pass, but if I have to buy a cat too then that just sucks. :) : : : Opinions?