# EGR? try disconnecting and plugging the vacuum line to the EGR. nm

Posted by Matt (93SE) on September 13, 2004 at 18:17:39: In Reply to: The Max Dies on Idle posted by xdannyx25 on September 11, 2004 at 16:41:47: : i put the new timing belt, everything went perfect, everythign lined up and still is lined up......but now ill start the car and i have to depress the pedal to open the throttle to keep it alive, if not itll just die out : -the coil and transistor are good, new spark plugs and wires. : -also i didnt put the a/c compressor in so theres one wire connector hanging, do you think thatll shut off the idle air control : -im thinking its the distributor lined up, cause when i match the dot and line on it, and place it in, the rotor is alittle past cyl 1 wire terminal. I have to push the distributor all the way to the right (driver side) to get it started. Replys:

Name: |
E-Mail |
Car: |
Subject |
Message:
: : i put the new timing belt, everything went perfect, everythign lined up and still is lined up......but now ill start the car and i have to depress the pedal to open the throttle to keep it alive, if not itll just die out : : -the coil and transistor are good, new spark plugs and wires. : : -also i didnt put the a/c compressor in so theres one wire connector hanging, do you think thatll shut off the idle air control : : -im thinking its the distributor lined up, cause when i match the dot and line on it, and place it in, the rotor is alittle past cyl 1 wire terminal. I have to push the distributor all the way to the right (driver side) to get it started.